Author: Steph Van Staden

Electric Furnaces

Furnace Technologies has been manufacturing furnaces in Western Australia since 1994. Our proven designs and attention to detail have set the standard for furnace manufacture. Our furnaces come in a variety of sizes and for different power requirements. All our furnaces are available in standard and HP (high powered) models to suit power availability and loads.
Our electric furnaces can also be fitted with a number of optional features to suit your requirements.
Custom sizes can be designed and manufactured on request.

Detail	Standard	Options
Shell	PGI	Stainless Steel
Thermocouples	Type K	Type R
Roof Style	Flat	Arched
Door hinge	LHS	Vertical or RHS
Over Temperature Protection	No	Thermal fuse or Control TC
Control	Single program	TAIE/Shinko multi program/ / Bartlett Genesis 2.0 touch screen

Electric Furnace Optional Features

CONTACT US

P: +61 8 9417 4226
E-Mail: sales@furnace-technologies.com.au
www.furnace-technologies.com.au

Furnace Technologies Pty Ltd
60 Cutler Road, Jandakot, WA 6164

Electric Furnaces

Standard Electric Furnace Specifications

Furnace	Internal mm			External mm			Power kw	Phase/ Amp	Max Temp
Model	W	D	H	W	D	H
C10	225	225	225	450	485	510	2.4	1/10	1100C
C14	330	330	330	750	540	580	2.4	1/10	1100C
P14	330	330	330	750	540	580	3.6	1/15	1250C
C27	380	380	460	950	775	795	3.6	1/15	1100C
P27S	380	380	460	950	775	795	4.8	1/20	1280C
P52S	490	490	610	1060	985	1620	9.2	3/15	1280C
P52HP	490	490	610	1060	985	1620	10.8	3/15	1280C
P80S	610	610	610	1180	1060	1615	10.8	3/15	1280C
P80HP	610	610	610	1180	1060	1615	14	3/20	1280C
P90S	610	610	760	1180	1060	1780	13.7	3/20	1280C
P90HP	610	610	760	1180	1060	1780	18.0	3/25	1280C
P100S	610	610	835	1180	1060	1780	15.3	3/23.3	1280C
P100HP	610	610	835	1180	1060	1780	18.2	3/27.5	1280C
P120S	610	610	910	1200	1060	1780	16.8	3/26.7	1280C
P120HP	610	610	910	1200	1060	1780	20	3/29.2	1280C
P160S	850	850	1200	1500	1460	2200	29	3/45	1280C
P160HP	850	850	1200	1500	1460	2200	36.2	3/55	1280C

CONTACT US

P: +61 8 9417 4226
E-Mail: sales@furnace-technologies.com.au
www.furnace-technologies.com.au

Furnace Technologies Pty Ltd
60 Cutler Road, Jandakot, WA 6164

Furnace Technologies Pty Ltd
60 Cutler Road, Jandakot, WA 6164

Electric Furnaces

Electric Kilns

We offer a select range of high quality controllers for Furnaces. This allows you to choose an option that offers the programming specifications, functions and interface that best fit your needs and provide the desired degree of control of the firing process.

FY 400

FY 700

TAIE Temperature Controllers

Digital PID Controller
Single (FY 400) or 18 program (FY 700)
8 steps in each program

Shinko PCB Temperature Controller

Digital PID Controller
10 program
10 steps in each program

CONTACT US

P: +61 8 9417 4226
E-Mail: sales@furnace-technologies.com.au
www.furnace-technologies.com.au

FT Touch Screen Control Box featuring
Bartlett Genesis 2.0 Controller
User-friendly touch screen interface for simple and effective operation
30 recipes /programs
Up to 32 steps in each recipe
Monitor your firing via PC or phone app
Pre-programmed with standard Bisque and Glost firing patterns, additional programs or adjustments to parameters available on request.

Furnace Technologies Pty Ltd
60 Cutler Road, Jandakot, WA 6164